Matching

“A” “B”

1. Use to connect two different network A. Active Directory
2. Regenerate Signal on a single network B. NIC
3. Layer 2 device that is used to expand existing C. Geteway

Network.

1. Prepare Data For transmission Between workstation D. CMOS
2. Stores Information about objects in network. E. Repeter
3. Parameter used in a network to determine F. Bridges

Data transfer mode.

1. An O layer that makes sure reliable transmission of data. G. Bandwidth of cable.
2. Provide high speed data transmission. H. Baseband.
3. An OSI layer used to convert data delivered by the sending I. Transport layer

Application layer in to universal accepted format.

1. Transport protocol used for unreliable data delivery. J. DMA channel
2. The principle of executing more than one application k. Data link layer

At a time.

1. A method of switching technology that opens communication L. Circuit Switching

Lines for a long as transmission time like telephone system.

1. Used to hold setting of Bios M. Serial transmission
2. Local Storage area with in the process that used to hold N. Registry

Data that is being worked on by the processor.

1. System pathway used by device to transfer information directly O. parallel transmission

To and from the memory. P. Session layer

Q. presentation layer

R. UDP

S. TCP

T. Multitasking

U. Leased Line

V. Wireless Channel

Answers

Matching

1. C 2. E 3. F 4. B 5. A 6. G 7. I 8. O 9. Q 10. R 11. T 12. L 13. D 14. N 15. J